1.  Make sure that your USB pendrive is FAT32 format
2.  ECMWHL0G.zip
3.  Copy efi folder and other files AfuEfix64.efi, ECMWHL0G.bin and update.nsh into root    
    directory of USB pendrive
4.  Execute update.nsh for automatic BIOS update. 