* **All BMC settings will be loaded default settings, including LAN settings and SEL records. Please make a backup first.**

### BMC update in Windows

1. Copy update tool and BMC file to windows.
2. Switch to the ipmi tool folder and double click **Flash.bat.**

Please wait. This may take few minutes.

一張含有 文字, 螢幕擷取畫面, 字型, 數字 的圖片

自動產生的描述

1. When the update process finishs, BMC will reset.

一張含有 文字, 螢幕擷取畫面, 陳列 的圖片

自動產生的描述

1. Wait three minute for BMC reset, run **chkver.bat** to check BMC firmware version.

一張含有 文字, 螢幕擷取畫面, 字型 的圖片

自動產生的描述