•	All BMC settings will be loaded default settings, including LAN settings and SEL records. Please make a backup first.

BMC update in Windows
1.	Copy update tool and BMC file to windows.

2.	Switch to the ipmi tool folder and double click “recovery.bat”.
Please wait. This may take few minutes.

3.	When the update process finishs, BMC will reset. 

4.	Wait three minutes for BMC reset, then reboot system to enter BIOS “Server Mgmt” page.
Make sure "BMC Self Test Status" is PASSED.
Make sure "BMC Firmware Revision" is the updated version.

