Flash steps:
1. Format your USB flash drive in FAT32 
2. Unzip ECMRPL0G.zip
3. Copy all the files of ECMRPL0G into USB flash drive
4. Under root directory of USB flash drive(For example, fs0:)
5. Type update.nsh for automatic BIOS flash
..