
Flash steps:
1. Format your USB flash drive in FAT32 
2. Unzip EPCADN04.ZIP
3. Copy all the files of EPCADN04 into a USB flash drive
4. Under root directory of USB flash drive(For example, fs0:)
5. Type update.nsh for automatic BIOS flash

.