


Step 1: Try to format your USB pen drive in FAT32 File System




Step 2: Unzip the BIOS ECMWHL0M.ZIP(for reference only. Please check the exact file name on your hands) and put all the files into the USB pen drive



Step 3: Press F11 on your keyboard to select a booting device. In this case, the second one is the device for USB pen drive and this is the one that we would pick up



Step 4: In general, fs1 represents USB pen drive while fs0 is usually for SSD/HDD device connecting the board



Step5: Type the command update.nsh and the script file will execute the BIOS update and flash the remaining process

